Alimentation/voeding

 **Features:**

**Constant Voltage Design**

**Class 2 power unit  Withstand Voltage I/P-O/P: 3kVAC**

**Protection:Short circuit,Overload,Over voltage,Over temperature  Safety: EN60950
 EMC Emission: EN55022 EN61000-3-2 EN61000-3-3  EMC Immunity: EN61000-4-2,3,4,5,6,8,11 EN55024**

**IP67 design for indoor or outdoor installations   100% full load burn-in test**

**3 years warranty
 **

**Ref : 812015**

**IP67**

**12V – 15W**



--------------------------------------------------------------------------------------------------------------------------------------

**Ref : 812030**

**IP67**

**12V-30W**

--------------------------------------------------------------------------------------------------------------------------------------

**Ref : 812060**

**IP65**

**12V – 60W**

--------------------------------------------------------------------------------------------------------------------------------------

**Ref : 824601**

**24V – 60W**

**Din**

**---------------------------------------------------------------------------------------------------------------------------**

**Ref : 824101**

**24V – 100W**

**Din**

**Ref : 824045**

**IP67**

**24V – 45W**

**---------------------------------------------------------------------------------------------------------------------------**

**Ref : 824100**

**IP 67**

**24V – 100W**

