Digital video recorder 32ch

|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
|  |  |  |  |  |  |  |
| **Model** | **9432LM** | | | | | |
|
| **System** | Main processor | Industrial-grade embedded HiSilicon CPU | | | | |
| Operating system | embedded Linux | | | | |
| System resources | Simultaneously multi-channel real-time recording, playback, network operation, USB backup | | | | |
| **Interface** | Operator interface | support 16-bit true color graphical menu interface and mouse operation | | | | |
| Preview | 1/4 /9/16/24/32split screen | | | | |
| **Video** | Codec | H.264（High Profile） | | | | |
| Monitor quality | VGA；HDMI：HD | | | | |
| Playback quality | AHD-M | | | | |
| Encode ability | 32\*AHD-M | | | | |
| Decode ability | 16\*AHD-M | | | | |
| Multi-mode input | 32\*AHD-M ；32\*CVBS | | | | |
| hybrid：4\*AHD-+4\*720P (network) | | | | |
| Network only：1\*1080P+8\*720P、4\*1080P | | | | |
| Motion Detection | Each screen can be set to 192 (16 \* 12) detection areas; multi-level sensitivity can be set (Limited local channel) | | | | |
| **Audio** | G.711A | | | | | |
| **Intercom** | support | | | | | |
| **Record & playback** | Record mode | manual>alarm>motion detection>timing | | | | |
| Local Playback | 16ch(local input mode) | | | | |
| Search mode | Search by time, calendar, event, channel | | | | |
| **Storage & backup** | Video storage | HDD, network | | | | |
| Backup mode | Network, USB hard disk, USB burner, SATA burner | | | | |
| **External Interface** | Video input | 32ch BNC | | | | |
| Video output | 1ch VGA, 1ch HDMI | | | | |
| Audio input | 16CH RCA | | | | |
| Audio output | 1CH RCA | | | | |
| Alarm input | 8CH | | | | |
| Alarm output | 1CH | | | | |
| Network interface | RJ45 10M/100M self-adaption | | | | |
| PTZ control | 1\*RS485, Support kinds of PTZ protocols | | | | |
| USB | 2\* USB 2.0 ports | | | | |
| HDD | 4\*SATA ports (Max 6TB/per) | | | | |
| Wireless | 3G, WIFI (extend via USB) | | | | |
| **General** | Power supply | 12V/6A | | | | |
| Power Consumption | <15W (without HDD) | | | | |

Ref999803